**MYERS AUTOMOTIVE DEMOLITION DERBY**

**Friday, August 19, 2022 at 7:00 p.m.**

**Chairperson: Mike Ladouceur 613-857-6766 mikeladouceur16@hotmail.com**

\*\*Cars on site by 6:00pm\*\* \*\*MANDATORY drivers meeting 6:45pm\*\* \*\* 7:00pm sharp start\*\*

GENERAL GUIDELINES

-Everybody must pay gate admission to gain access to grounds

-No persons under the age of 16 are allowed in the pit area at any time

-All drivers must have a valid G2 class over above drivers license as of the date of the derby.

NO EXCEPTIONS

-Only driver plus ONE other person allowed in pit area

-NO ALCOHOL PERMITTED ON GROUNDS. OPP enforced

PRIZE MONEY

-Overall class winner: $600.00 per class

-Overall class runner up: $300.00 per class

-Heat winners (2 per heat): $100.00 each

\*\*\*MTAS will not be held responsible for any vehicles, parts, personal property, or injury before, during, or after the event. In the interest of safety, anyone entering is subject to and must obey the following rules and regulations\*\*\*\*

RULES AND REGULATIONS

-Each driver must fill out an entry form

-Each driver must have at least a G2 license and present the valid license upon arrival

-Each driver must supply their own vehicle and arrive with it derby ready

-MTAS reserves the right to approve or reject any or all entries

-No vehicles are permitted in the competition area before the heat in which they are to participate

-All drivers must attend a MANDATORY driver meeting before the commencement of the event

-Failure to comply with the rules and regulations is grounds for disqualification without refund

TYPE OF VEHICLE

-Any stock, hardtop automobile or station wagon is allowed

-Any stock, factory made rear ends are permitted, including posi-traction and limited slip differentials

-No trucks, jeeps, convertibles, hearses, or limousines are allowed.

PREPARATION OF VEHICLE  
-The following must be removed before arriving at the fairgrounds:

-All glass (including windshield, side windows, head and taillights; \*\*rolling down window is not permitted\*\*)

-All airbags

-Chrome molding strips and bottom portion of rear seat (mash down or cut off)

-Special bumpers, reinforcements, fabrications, trailer hitches, etc.

-Welded solid or chained-down engine mounts are recommended

-Roll over bars are allowed but not necessary

-All doors must be fastened shut by minimum four (4) strands of wire, straps, or welded

-No spring jacks, blocked shocks, or reversed shackles are permitted

-Suspension must be free of blocks. Helper springs or altered suspensions are not permitted and torsion bars must be at manufacturer’s specifications

-Only one automotive-type battery is allowed. It may be relocated to any location in the car, but MUST be **securely fastened and covered**

-Cutting fenders for wheel clearance only is permissible- ends of bumpers may be cut off

-Hood must be fastened down in four (4) places; trunk or tailgate must be fastened down in four (4) places. \*\*Official’s decision on overuse of wire\*\*

-Stock gas tanks must be moved from stock position into trunk or rear seat area. A small, portable tank is recommended in place of the original.

-All tanks must be securely **fastened and covered**

-Maximum of four (4) gallons of fuel is permitted per heat

-ABSOLUTELY NO PLASTIC FUEL CANS ARE PERMITTED

-Vehicle must be swept clean; absolutely no junk tires, wheels, metal parts, glass, etc. is allowed in the vehicle

-It is recommended that the driver’s door be reinforced inside with steel bar, angle iron or pipe

-Length not to extend more than eight (8) inches on either end of the driver’s door

-It is recommended that a minimum sixteen (16) inch opening be cut in the centre of the hood cover over the carburetor in case of fire

-No double tires permitted- automotive only

-No studs or screws in rims to hold tires

-Strong wire or nylon mesh screen is recommended on driver’s window and windshield area

-Scatter shields are also recommended

DRIVER SAFETY APPAREL

\*\*Drivers will not be permitted to compete without all safety apparel\*\*

\*\*Z-90 safety belt, approved helmet and approved goggles for eye protection are mandatory. One piece overalls or garment with long sleeves and pant legs. NO SHORTS ARE PERMITTED\*\*

RUNNING

-Drivers may maneuver forward and backward, but deliberate hitting on driver’s door can be cause for disqualification

-Vehicles must always have dependable and sufficient brakes

-Competition area boundaries must be observed at all times

-Vehicles who fail to stay in the confines of the competition area will be disqualified

ABSOLUTELY NO ALCOHOL OR DRUGS WILL BE PERMITTED ON GROUNDS

- Drivers or pit crew who are in possession of or under the influence of drugs or alcohol will be disqualified

-A vehicle will be disqualified if the driver’s door comes open during a heat

-A 60 second time limit is enforced by officials for restarts and making competitive contact with another vehicle

-Simple hits do not constitute combat and could be considered sandbagging

-Hits must be aggressive

-All heat winners will be allowed to work on their cars for 20 minutes before the final heat

-The air horn will signal the start and stop of heats

-If at any time during the heat the air horn sounds, all vehicles must stop

-Failure to do so will result in immediate disqualification

-If at any point a vehicle becomes a safety hazard, the derby coordinator and/or the fire department reserve the right to eject the driver and vehicle from the competition

ALL VEHICLES MUST BE REMOVED FROM THE MTAS GROUNDS IMMEDIATELY FOLLOWING THE EVENT. VEHICLES LEFT ON GROUNDS WILL BECOME PROPERTY OF MTAS AND WILL BE REMOVED. TITLES MUST BE TURNED IN ON ALL CARS LEFT FOR JUNK